| 6. Adjusting the confocality of the TV adapter In the case of U-TV0.5XC | Basics |

| Switch to an objective with as high a magnification as possible.
| Bring a specimen into focus while looking through the eyepiece.
| Switch to the objective with the lowest magnification.
| Loosen the screw (LOCK) using a Allen screwdriver.
| While viewing the specimen on the monitor, bring it into focus by turning the screw (FOCUS) with the Allen screwdriver.
| When the specimen has been brought into focus, tighten the screw (LOCK).
| (If you use a TV adapter other than the U-TV0.5XC, refer to the instruction manual for the TV adapter that you use.)
|  | What is confocal adjustment?: The eyepiece and camera are adjusted so that the image in focus viewed through the eyepiece is confocal with the image in focus viewed through the camera. |
|  |  | 7