| Auto Exposure (AE) Compensation procedure | Appli- cations |

| Select the “REC AUTO” mode using the MODE button.
| While viewing an image, correct the automatically set exposure time using the right and left buttons. The right key (+) is for lengthening the exposure time to acquire a bright image. The left key (-) is for shortening the exposure time to acquire a dark image.
| The set value can be checked on the INFO screen. |
| Press the EXPOSE button to acquire the image.
|  |  | 17