| Display to scale - 1 | Appli- cations |

|  | The scale of a magnification used for a specimen can be overlaid on an image being observed. The scale can be displayed in the two ways shown below.
| The scale is displayed on both a live image and an acquired image.
| The scale is displayed only on a live image.
When one objective is switched to another, the scale is also automatically switched to the one appropriate for the magnification of the new objective.
|  | To display the scale appropriate for the magnification of an objective, it is necessary to input data on the magnifications of the objective and TV adapter you use into the DP21/DP26. For information on how to input them into the DP21/DP26, refer to the instruction manual. |
|  |  | 18